GENERAL DATA	
 					
 COMPUTING METHOD					
 					
 x Structural Analysis		x 1st Order Analysis			
   Stress Analysis		  2nd Order Analysis			
   Dynamic Analysis		  Cable Theory			
 					
 x Load Cases		  Design Cases			
   Load Groups		  Dynamic Cases			
   Load Combinations		  Buckling Curves			
 					
 STRUCTURAL DATA  PARAMETERS					
 					
   1D Continuous Beam	10	Nodes	15	Elements	
 x 2D Construction Type	2	Materials	0	Cables	
   3D Construction Type	3	Sections	0	Tapered Elements	
   Grid	0	Element Hinges	0	Elastic Foundations	
 	0	Element Partitions	0	Sets of Elements	

NODES	
 Node	Coordinates-	Ref	Node Coordinates	
 No	System	Nodes	X [m]	Y [m]	Z [m]	
 1	Cartesian	-	0.000		0.000	
 	Supported	
 2	Cartesian	-	0.000		5.417	
 	Supported	
 4	Cartesian	-	4.817		0.000	
 5	Cartesian	-	4.817		5.417	
 7	Cartesian	-	9.750		0.000	
 8	Cartesian	-	9.750		5.417	
 10	Cartesian	-	14.683		0.000	
 11	Cartesian	-	14.683		5.417	
 13	Cartesian	-	19.500		0.000	
 	Supported	
 14	Cartesian	-	19.500		5.417	
 	Supported	

MATERIALS	
 Mat	Material	E Modulus	Shear Mod	Spec Weight	Coeff Therm	
 No	Description	[kN/mm^2]	[kN/mm^2]	[kN/mm^3]	[1/°C]	
 1	GL28c	1.260E+01	7.200E-01	3.800E-09	5.000E-06	
 2	Fe 360 B	2.100E+02	8.100E+01	7.850E-08	1.200E-05	

SECTIONS	
 Sec	Mat	Section	I-2	A	A-3	
 No	No	Description	[mm^4]	[mm^2]	[mm^2]	
 1	1	Rectangle 900/160	307200000.	144000.0		
 2	1	Rectangle 240/160	81920000.	38400.0		
 3	2	Round 20	7854.	314.2		

ELEMENTS	
 Elem	Elem	Nodes	Beta	Section	Hinge	Part	Length	Elem	
 No	Type	Begin	End	[°]	Begin	End	Begin	End	No	[m]	Location	
 4	Beam	1	4	0.00	1	1	-	-	-	4.817	HORI	
 5	Beam	2	5	0.00	1	1	-	-	-	4.817	HORI	
 8	Truss	4	5	0.00	2	2	-	-	-	5.417	VERT	
 11	Beam	4	7	0.00	1	1	-	-	-	4.933	HORI	
 12	Beam	5	8	0.00	1	1	-	-	-	4.933	HORI	
 15	Truss	8	7	0.00	2	2	-	-	-	5.417	VERT	
 18	Beam	7	10	0.00	1	1	-	-	-	4.933	HORI	
 19	Beam	8	11	0.00	1	1	-	-	-	4.933	HORI	
 22	Truss	10	11	0.00	2	2	-	-	-	5.417	VERT	
 25	Beam	10	13	0.00	1	1	-	-	-	4.817	HORI	
 26	Beam	11	14	0.00	1	1	-	-	-	4.817	HORI	
 27	Truss	2	4	0.00	3	3	-	-	-	7.249	GENL	
 29	Truss	5	7	0.00	3	3	-	-	-	7.326	GENL	
 32	Truss	7	11	0.00	3	3	-	-	-	7.326	GENL	
 34	Truss	10	14	0.00	3	3	-	-	-	7.249	GENL	

SUPPORTS	
 Support	Supported	Rotation [°]	Fixed Support/Support Spring [kN/m] [kNm/rad]	
 No	Nodes	Alpha	Beta	in X	in Y	in Z	ar X	ar Y	ar Z	
 1	2	0.0	0.0	Yes		Yes		No		
 2	1,13,14	0.0	0.0	No		Yes		No		

GENERAL DATA	
 LC No	LC Description	Factor	Combination Type	Dead Weight	
 1	Sbandamento permanenti	1.00	Permanent	-	
 2	Sbandamento accidentali	1.00	Permanent	-	
 3	Sisma	1.00	Permanent	-	

ELEMENT LOADS	LC 1	
 	Loaded	Load	Load	Parameters [kN, kNm, m, °C, kN/m, kNm/m]	
 No	Elements	type	Direction	P-1				
 1	5,12,19,26	1	Z	-0.081				

ELEMENT LOADS	LC 2	
 	Loaded	Load	Load	Parameters [kN, kNm, m, °C, kN/m, kNm/m]	
 No	Elements	type	Direction	P-1				
 1	5,12,19,26	1	Z	-0.107				

ELEMENT LOADS	LC 3	
 	Loaded	Load	Load	Parameters [kN, kNm, m, °C, kN/m, kNm/m]	
 No	Elements	type	Direction	P-1				
 1	5,12,19,26	1	Z	-1.726				

INTERNAL FORCES BY ELEMENT	
 Elem	LC/LG 	Node	x	Forces [kN]	Moments [kNm]	
 No	No	No	[m]	N	V-2	V-3	T	M-2	M-3	
     4	LC1	      1	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		      4	   4.82	     .00	     .00	     .00	     .00	     .02	     .00	
      		Max  N 	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		Min  N 	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		Max V-3	   4.82	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min V-3	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		Max M-2	   4.82	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      	LC2	      1	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		      4	   4.82	     .00	     .00	     .00	     .00	     .02	     .00	
      		Max  N 	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		Min  N 	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		Max V-3	   4.82	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min V-3	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      		Max M-2	   4.82	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	    .00	     .00	     .00	     .00	     .00	     .00	     .00	
      	LC3	      1	    .00	     .00	     .00	     .07	     .00	     .00	     .00	
      		      4	   4.82	     .00	     .00	     .07	     .00	     .35	     .00	
      		Max  N 	    .00	     .00	     .00	     .07	     .00	     .00	     .00	
      		Min  N 	    .00	     .00	     .00	     .07	     .00	     .00	     .00	
      		Max V-3	    .00	     .00	     .00	     .07	     .00	     .00	     .00	
      		Min V-3	    .00	     .00	     .00	     .07	     .00	     .00	     .00	
      		Max M-2	   4.82	     .00	     .00	     .07	     .00	     .35	     .00	
      		Min M-2	    .00	     .00	     .00	     .07	     .00	     .00	     .00	
     5	LC1	      2	    .00	    -.56	     .00	     .16	     .00	     .00	     .00	
      		      5	   4.82	    -.56	     .00	    -.23	     .00	    -.18	     .00	
      		Max  N 	   4.82	    -.56	     .00	    -.23	     .00	    -.18	     .00	
      		Min  N 	    .00	    -.56	     .00	     .16	     .00	     .00	     .00	
      		Max V-3	    .00	    -.56	     .00	     .16	     .00	     .00	     .00	
      		Min V-3	   4.82	    -.56	     .00	    -.23	     .00	    -.18	     .00	
      		Max M-2	   1.93	    -.56	     .00	     .00	     .00	     .15	     .00	
      		Min M-2	   4.82	    -.56	     .00	    -.23	     .00	    -.18	     .00	
      	LC2	      2	    .00	    -.74	     .00	     .21	     .00	     .00	     .00	
      		      5	   4.82	    -.74	     .00	    -.31	     .00	    -.24	     .00	
      		Max  N 	    .00	    -.74	     .00	     .21	     .00	     .00	     .00	
      		Min  N 	    .00	    -.74	     .00	     .21	     .00	     .00	     .00	
      		Max V-3	    .00	    -.74	     .00	     .21	     .00	     .00	     .00	
      		Min V-3	   4.82	    -.74	     .00	    -.31	     .00	    -.24	     .00	
      		Max M-2	   1.93	    -.74	     .00	     .00	     .00	     .20	     .00	
      		Min M-2	   4.82	    -.74	     .00	    -.31	     .00	    -.24	     .00	
      	LC3	      2	    .00	  -11.93	     .00	    3.34	     .00	     .00	     .00	
      		      5	   4.82	  -11.93	     .00	   -4.97	     .00	   -3.93	     .00	
      		Max  N 	    .00	  -11.93	     .00	    3.34	     .00	     .00	     .00	
      		Min  N 	    .00	  -11.93	     .00	    3.34	     .00	     .00	     .00	
      		Max V-3	    .00	  -11.93	     .00	    3.34	     .00	     .00	     .00	
      		Min V-3	   4.82	  -11.93	     .00	   -4.97	     .00	   -3.93	     .00	
      		Max M-2	   1.93	  -11.93	     .00	     .02	     .00	    3.23	     .00	
      		Min M-2	   4.82	  -11.93	     .00	   -4.97	     .00	   -3.93	     .00	
     8	LC1	      4	    .00	    -.63	     .00	     .00				
      		      5	   5.42	    -.63	     .00	     .00				
      		Max  N 	    .00	    -.63	     .00	     .00				
      		Min  N 	    .00	    -.63	     .00	     .00				
      		Max V-3	    .00	    -.63	     .00	     .00				
      		Min V-3	    .00	    -.63	     .00	     .00				
      	LC2	      4	    .00	    -.84	     .00	     .00				
      		      5	   5.42	    -.84	     .00	     .00				
      		Max  N 	    .00	    -.84	     .00	     .00				
      		Min  N 	    .00	    -.84	     .00	     .00				
      		Max V-3	    .00	    -.84	     .00	     .00				
      		Min V-3	    .00	    -.84	     .00	     .00				
      	LC3	      4	    .00	  -13.50	     .00	     .00				
      		      5	   5.42	  -13.50	     .00	     .00				
      		Max  N 	    .00	  -13.50	     .00	     .00				
      		Min  N 	    .00	  -13.50	     .00	     .00				
      		Max V-3	    .00	  -13.50	     .00	     .00				
      		Min V-3	    .00	  -13.50	     .00	     .00				
    11	LC1	      4	    .00	     .56	     .00	     .00	     .00	     .02	     .00	
      		      7	   4.93	     .56	     .00	     .00	     .00	     .01	     .00	
      		Max  N 	    .00	     .56	     .00	     .00	     .00	     .02	     .00	
      		Min  N 	    .00	     .56	     .00	     .00	     .00	     .02	     .00	
      		Max V-3	   4.93	     .56	     .00	     .00	     .00	     .01	     .00	
      		Min V-3	    .00	     .56	     .00	     .00	     .00	     .02	     .00	
      		Max M-2	    .00	     .56	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	   4.93	     .56	     .00	     .00	     .00	     .01	     .00	
      	LC2	      4	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		      7	   4.93	     .74	     .00	     .00	     .00	     .02	     .00	
      		Max  N 	   4.93	     .74	     .00	     .00	     .00	     .02	     .00	
      		Min  N 	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		Max V-3	   4.93	     .74	     .00	     .00	     .00	     .02	     .00	
      		Min V-3	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		Max M-2	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	   4.93	     .74	     .00	     .00	     .00	     .02	     .00	
      	LC3	      4	    .00	   11.93	     .00	    -.01	     .00	     .35	     .00	
      		      7	   4.93	   11.93	     .00	    -.01	     .00	     .31	     .00	
      		Max  N 	   4.93	   11.93	     .00	    -.01	     .00	     .31	     .00	
      		Min  N 	    .00	   11.93	     .00	    -.01	     .00	     .35	     .00	
      		Max V-3	   4.93	   11.93	     .00	    -.01	     .00	     .31	     .00	
      		Min V-3	    .00	   11.93	     .00	    -.01	     .00	     .35	     .00	
      		Max M-2	    .00	   11.93	     .00	    -.01	     .00	     .35	     .00	
      		Min M-2	   4.93	   11.93	     .00	    -.01	     .00	     .31	     .00	
    12	LC1	      5	    .00	    -.73	     .00	     .21	     .00	    -.18	     .00	
      		      8	   4.93	    -.73	     .00	    -.19	     .00	    -.13	     .00	
      		Max  N 	   4.93	    -.73	     .00	    -.19	     .00	    -.13	     .00	
      		Min  N 	    .00	    -.73	     .00	     .21	     .00	    -.18	     .00	
      		Max V-3	    .00	    -.73	     .00	     .21	     .00	    -.18	     .00	
      		Min V-3	   4.93	    -.73	     .00	    -.19	     .00	    -.13	     .00	
      		Max M-2	   2.71	    -.73	     .00	    -.01	     .00	     .09	     .00	
      		Min M-2	    .00	    -.73	     .00	     .21	     .00	    -.18	     .00	
      	LC2	      5	    .00	    -.97	     .00	     .28	     .00	    -.24	     .00	
      		      8	   4.93	    -.97	     .00	    -.25	     .00	    -.18	     .00	
      		Max  N 	    .00	    -.97	     .00	     .28	     .00	    -.24	     .00	
      		Min  N 	    .00	    -.97	     .00	     .28	     .00	    -.24	     .00	
      		Max V-3	    .00	    -.97	     .00	     .28	     .00	    -.24	     .00	
      		Min V-3	   4.93	    -.97	     .00	    -.25	     .00	    -.18	     .00	
      		Max M-2	   2.71	    -.97	     .00	    -.01	     .00	     .12	     .00	
      		Min M-2	    .00	    -.97	     .00	     .28	     .00	    -.24	     .00	
      	LC3	      5	    .00	  -15.61	     .00	    4.48	     .00	   -3.93	     .00	
      		      8	   4.93	  -15.61	     .00	   -4.03	     .00	   -2.83	     .00	
      		Max  N 	    .00	  -15.61	     .00	    4.48	     .00	   -3.93	     .00	
      		Min  N 	    .00	  -15.61	     .00	    4.48	     .00	   -3.93	     .00	
      		Max V-3	    .00	  -15.61	     .00	    4.48	     .00	   -3.93	     .00	
      		Min V-3	   4.93	  -15.61	     .00	   -4.03	     .00	   -2.83	     .00	
      		Max M-2	   2.71	  -15.61	     .00	    -.20	     .00	    1.87	     .00	
      		Min M-2	    .00	  -15.61	     .00	    4.48	     .00	   -3.93	     .00	
    15	LC1	      8	    .00	    -.38	     .00	     .00				
      		      7	   5.42	    -.38	     .00	     .00				
      		Max  N 	   5.42	    -.38	     .00	     .00				
      		Min  N 	    .00	    -.38	     .00	     .00				
      		Max V-3	    .00	    -.38	     .00	     .00				
      		Min V-3	    .00	    -.38	     .00	     .00				
      	LC2	      8	    .00	    -.50	     .00	     .00				
      		      7	   5.42	    -.50	     .00	     .00				
      		Max  N 	    .00	    -.50	     .00	     .00				
      		Min  N 	    .00	    -.50	     .00	     .00				
      		Max V-3	    .00	    -.50	     .00	     .00				
      		Min V-3	    .00	    -.50	     .00	     .00				
      	LC3	      8	    .00	   -8.07	     .00	     .00				
      		      7	   5.42	   -8.07	     .00	     .00				
      		Max  N 	   5.42	   -8.07	     .00	     .00				
      		Min  N 	    .00	   -8.07	     .00	     .00				
      		Max V-3	    .00	   -8.07	     .00	     .00				
      		Min V-3	    .00	   -8.07	     .00	     .00				
    18	LC1	      7	    .00	     .56	     .00	     .00	     .00	     .01	     .00	
      		     10	   4.93	     .56	     .00	     .00	     .00	     .02	     .00	
      		Max  N 	    .00	     .56	     .00	     .00	     .00	     .01	     .00	
      		Min  N 	    .00	     .56	     .00	     .00	     .00	     .01	     .00	
      		Max V-3	   4.93	     .56	     .00	     .00	     .00	     .02	     .00	
      		Min V-3	    .00	     .56	     .00	     .00	     .00	     .01	     .00	
      		Max M-2	   4.93	     .56	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	    .00	     .56	     .00	     .00	     .00	     .01	     .00	
      	LC2	      7	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		     10	   4.93	     .74	     .00	     .00	     .00	     .02	     .00	
      		Max  N 	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		Min  N 	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		Max V-3	   4.93	     .74	     .00	     .00	     .00	     .02	     .00	
      		Min V-3	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      		Max M-2	   4.93	     .74	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	    .00	     .74	     .00	     .00	     .00	     .02	     .00	
      	LC3	      7	    .00	   11.93	     .00	     .01	     .00	     .31	     .00	
      		     10	   4.93	   11.93	     .00	     .01	     .00	     .35	     .00	
      		Max  N 	   4.93	   11.93	     .00	     .01	     .00	     .35	     .00	
      		Min  N 	    .00	   11.93	     .00	     .01	     .00	     .31	     .00	
      		Max V-3	   4.93	   11.93	     .00	     .01	     .00	     .35	     .00	
      		Min V-3	    .00	   11.93	     .00	     .01	     .00	     .31	     .00	
      		Max M-2	   4.93	   11.93	     .00	     .01	     .00	     .35	     .00	
      		Min M-2	    .00	   11.93	     .00	     .01	     .00	     .31	     .00	
    19	LC1	      8	    .00	    -.73	     .00	     .19	     .00	    -.13	     .00	
      		     11	   4.93	    -.73	     .00	    -.21	     .00	    -.18	     .00	
      		Max  N 	   4.93	    -.73	     .00	    -.21	     .00	    -.18	     .00	
      		Min  N 	    .00	    -.73	     .00	     .19	     .00	    -.13	     .00	
      		Max V-3	    .00	    -.73	     .00	     .19	     .00	    -.13	     .00	
      		Min V-3	   4.93	    -.73	     .00	    -.21	     .00	    -.18	     .00	
      		Max M-2	   2.22	    -.73	     .00	     .01	     .00	     .09	     .00	
      		Min M-2	   4.93	    -.73	     .00	    -.21	     .00	    -.18	     .00	
      	LC2	      8	    .00	    -.97	     .00	     .25	     .00	    -.18	     .00	
      		     11	   4.93	    -.97	     .00	    -.28	     .00	    -.24	     .00	
      		Max  N 	    .00	    -.97	     .00	     .25	     .00	    -.18	     .00	
      		Min  N 	    .00	    -.97	     .00	     .25	     .00	    -.18	     .00	
      		Max V-3	    .00	    -.97	     .00	     .25	     .00	    -.18	     .00	
      		Min V-3	   4.93	    -.97	     .00	    -.28	     .00	    -.24	     .00	
      		Max M-2	   2.22	    -.97	     .00	     .01	     .00	     .12	     .00	
      		Min M-2	   4.93	    -.97	     .00	    -.28	     .00	    -.24	     .00	
      	LC3	      8	    .00	  -15.61	     .00	    4.03	     .00	   -2.83	     .00	
      		     11	   4.93	  -15.61	     .00	   -4.48	     .00	   -3.93	     .00	
      		Max  N 	    .00	  -15.61	     .00	    4.03	     .00	   -2.83	     .00	
      		Min  N 	    .00	  -15.61	     .00	    4.03	     .00	   -2.83	     .00	
      		Max V-3	    .00	  -15.61	     .00	    4.03	     .00	   -2.83	     .00	
      		Min V-3	   4.93	  -15.61	     .00	   -4.48	     .00	   -3.93	     .00	
      		Max M-2	   2.22	  -15.61	     .00	     .20	     .00	    1.87	     .00	
      		Min M-2	   4.93	  -15.61	     .00	   -4.48	     .00	   -3.93	     .00	
    22	LC1	     10	    .00	    -.63	     .00	     .00				
      		     11	   5.42	    -.63	     .00	     .00				
      		Max  N 	    .00	    -.63	     .00	     .00				
      		Min  N 	    .00	    -.63	     .00	     .00				
      		Max V-3	    .00	    -.63	     .00	     .00				
      		Min V-3	    .00	    -.63	     .00	     .00				
      	LC2	     10	    .00	    -.84	     .00	     .00				
      		     11	   5.42	    -.84	     .00	     .00				
      		Max  N 	    .00	    -.84	     .00	     .00				
      		Min  N 	    .00	    -.84	     .00	     .00				
      		Max V-3	    .00	    -.84	     .00	     .00				
      		Min V-3	    .00	    -.84	     .00	     .00				
      	LC3	     10	    .00	  -13.50	     .00	     .00				
      		     11	   5.42	  -13.50	     .00	     .00				
      		Max  N 	    .00	  -13.50	     .00	     .00				
      		Min  N 	    .00	  -13.50	     .00	     .00				
      		Max V-3	    .00	  -13.50	     .00	     .00				
      		Min V-3	    .00	  -13.50	     .00	     .00				
    25	LC1	     10	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		     13	   4.82	     .00	     .00	     .00	     .00	     .00	     .00	
      		Max  N 	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min  N 	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Max V-3	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min V-3	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Max M-2	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	   4.82	     .00	     .00	     .00	     .00	     .00	     .00	
      	LC2	     10	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		     13	   4.82	     .00	     .00	     .00	     .00	     .00	     .00	
      		Max  N 	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min  N 	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Max V-3	   4.82	     .00	     .00	     .00	     .00	     .00	     .00	
      		Min V-3	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Max M-2	    .00	     .00	     .00	     .00	     .00	     .02	     .00	
      		Min M-2	   4.82	     .00	     .00	     .00	     .00	     .00	     .00	
      	LC3	     10	    .00	     .00	     .00	    -.07	     .00	     .35	     .00	
      		     13	   4.82	     .00	     .00	    -.07	     .00	     .00	     .00	
      		Max  N 	    .00	     .00	     .00	    -.07	     .00	     .35	     .00	
      		Min  N 	    .00	     .00	     .00	    -.07	     .00	     .35	     .00	
      		Max V-3	   4.82	     .00	     .00	    -.07	     .00	     .00	     .00	
      		Min V-3	    .00	     .00	     .00	    -.07	     .00	     .35	     .00	
      		Max M-2	    .00	     .00	     .00	    -.07	     .00	     .35	     .00	
      		Min M-2	   4.82	     .00	     .00	    -.07	     .00	     .00	     .00	
    26	LC1	     11	    .00	    -.56	     .00	     .23	     .00	    -.18	     .00	
      		     14	   4.82	    -.56	     .00	    -.16	     .00	     .00	     .00	
      		Max  N 	   4.82	    -.56	     .00	    -.16	     .00	     .00	     .00	
      		Min  N 	    .00	    -.56	     .00	     .23	     .00	    -.18	     .00	
      		Max V-3	    .00	    -.56	     .00	     .23	     .00	    -.18	     .00	
      		Min V-3	   4.82	    -.56	     .00	    -.16	     .00	     .00	     .00	
      		Max M-2	   2.89	    -.56	     .00	     .00	     .00	     .15	     .00	
      		Min M-2	    .00	    -.56	     .00	     .23	     .00	    -.18	     .00	
      	LC2	     11	    .00	    -.74	     .00	     .31	     .00	    -.24	     .00	
      		     14	   4.82	    -.74	     .00	    -.21	     .00	     .00	     .00	
      		Max  N 	   4.82	    -.74	     .00	    -.21	     .00	     .00	     .00	
      		Min  N 	    .00	    -.74	     .00	     .31	     .00	    -.24	     .00	
      		Max V-3	    .00	    -.74	     .00	     .31	     .00	    -.24	     .00	
      		Min V-3	   4.82	    -.74	     .00	    -.21	     .00	     .00	     .00	
      		Max M-2	   2.89	    -.74	     .00	     .00	     .00	     .20	     .00	
      		Min M-2	    .00	    -.74	     .00	     .31	     .00	    -.24	     .00	
      	LC3	     11	    .00	  -11.93	     .00	    4.97	     .00	   -3.93	     .00	
      		     14	   4.82	  -11.93	     .00	   -3.34	     .00	     .00	     .00	
      		Max  N 	    .00	  -11.93	     .00	    4.97	     .00	   -3.93	     .00	
      		Min  N 	    .00	  -11.93	     .00	    4.97	     .00	   -3.93	     .00	
      		Max V-3	    .00	  -11.93	     .00	    4.97	     .00	   -3.93	     .00	
      		Min V-3	   4.82	  -11.93	     .00	   -3.34	     .00	     .00	     .00	
      		Max M-2	   2.89	  -11.93	     .00	    -.02	     .00	    3.23	     .00	
      		Min M-2	    .00	  -11.93	     .00	    4.97	     .00	   -3.93	     .00	
    27	LC1	      2	    .00	     .84	     .00	     .00				
      		      4	   7.25	     .84	     .00	     .00				
      		Max  N 	   7.25	     .84	     .00	     .00				
      		Min  N 	    .00	     .84	     .00	     .00				
      		Max V-3	    .00	     .84	     .00	     .00				
      		Min V-3	    .00	     .84	     .00	     .00				
      	LC2	      2	    .00	    1.11	     .00	     .00				
      		      4	   7.25	    1.11	     .00	     .00				
      		Max  N 	   7.25	    1.11	     .00	     .00				
      		Min  N 	    .00	    1.11	     .00	     .00				
      		Max V-3	    .00	    1.11	     .00	     .00				
      		Min V-3	    .00	    1.11	     .00	     .00				
      	LC3	      2	    .00	   17.95	     .00	     .00				
      		      4	   7.25	   17.95	     .00	     .00				
      		Max  N 	    .00	   17.95	     .00	     .00				
      		Min  N 	    .00	   17.95	     .00	     .00				
      		Max V-3	    .00	   17.95	     .00	     .00				
      		Min V-3	    .00	   17.95	     .00	     .00				
    29	LC1	      5	    .00	     .26	     .00	     .00				
      		      7	   7.33	     .26	     .00	     .00				
      		Max  N 	    .00	     .26	     .00	     .00				
      		Min  N 	    .00	     .26	     .00	     .00				
      		Max V-3	    .00	     .26	     .00	     .00				
      		Min V-3	    .00	     .26	     .00	     .00				
      	LC2	      5	    .00	     .34	     .00	     .00				
      		      7	   7.33	     .34	     .00	     .00				
      		Max  N 	    .00	     .34	     .00	     .00				
      		Min  N 	    .00	     .34	     .00	     .00				
      		Max V-3	    .00	     .34	     .00	     .00				
      		Min V-3	    .00	     .34	     .00	     .00				
      	LC3	      5	    .00	    5.47	     .00	     .00				
      		      7	   7.33	    5.47	     .00	     .00				
      		Max  N 	   7.33	    5.47	     .00	     .00				
      		Min  N 	    .00	    5.47	     .00	     .00				
      		Max V-3	    .00	    5.47	     .00	     .00				
      		Min V-3	    .00	    5.47	     .00	     .00				
    32	LC1	      7	    .00	     .26	     .00	     .00				
      		     11	   7.33	     .26	     .00	     .00				
      		Max  N 	   7.33	     .26	     .00	     .00				
      		Min  N 	    .00	     .26	     .00	     .00				
      		Max V-3	    .00	     .26	     .00	     .00				
      		Min V-3	    .00	     .26	     .00	     .00				
      	LC2	      7	    .00	     .34	     .00	     .00				
      		     11	   7.33	     .34	     .00	     .00				
      		Max  N 	   7.33	     .34	     .00	     .00				
      		Min  N 	    .00	     .34	     .00	     .00				
      		Max V-3	    .00	     .34	     .00	     .00				
      		Min V-3	    .00	     .34	     .00	     .00				
      	LC3	      7	    .00	    5.47	     .00	     .00				
      		     11	   7.33	    5.47	     .00	     .00				
      		Max  N 	   7.33	    5.47	     .00	     .00				
      		Min  N 	    .00	    5.47	     .00	     .00				
      		Max V-3	    .00	    5.47	     .00	     .00				
      		Min V-3	    .00	    5.47	     .00	     .00				
    34	LC1	     10	    .00	     .84	     .00	     .00				
      		     14	   7.25	     .84	     .00	     .00				
      		Max  N 	   7.25	     .84	     .00	     .00				
      		Min  N 	    .00	     .84	     .00	     .00				
      		Max V-3	    .00	     .84	     .00	     .00				
      		Min V-3	    .00	     .84	     .00	     .00				
      	LC2	     10	    .00	    1.11	     .00	     .00				
      		     14	   7.25	    1.11	     .00	     .00				
      		Max  N 	   7.25	    1.11	     .00	     .00				
      		Min  N 	    .00	    1.11	     .00	     .00				
      		Max V-3	    .00	    1.11	     .00	     .00				
      		Min V-3	    .00	    1.11	     .00	     .00				
      	LC3	     10	    .00	   17.95	     .00	     .00				
      		     14	   7.25	   17.95	     .00	     .00				
      		Max  N 	    .00	   17.95	     .00	     .00				
      		Min  N 	    .00	   17.95	     .00	     .00				
      		Max V-3	    .00	   17.95	     .00	     .00				
      		Min V-3	    .00	   17.95	     .00	     .00