NODES	
 Node	Coordinates-	Ref	Node Coordinates	
 No	System	Nodes	X [m]	Y [m]	Z [m]	
 1	Cartesian	-	0.000		0.000	
 	Supported	
 2	Cartesian	-	1.000		-2.355	
 3	Cartesian	-	4.845		-3.100	
 	Supported	
 4	Cartesian	-	0.200		-0.471	
 5	Cartesian	-	0.400		-0.942	
 6	Cartesian	-	0.600		-1.413	
 7	Cartesian	-	0.800		-1.884	
 8	Cartesian	-	1.769		-2.504	
 9	Cartesian	-	2.538		-2.653	
 10	Cartesian	-	3.307		-2.802	
 11	Cartesian	-	4.076		-2.951	

MATERIALS	
 Mat	Material	E Modulus	Shear Mod	Spec Weight	Coeff Therm	
 No	Description	[kN/cm^2]	[kN/cm^2]	[kN/cm^3]	[1/°C]	
 1	BS11, S10/MS10	1.100E+03	5.500E+01	5.000E-06	5.000E-06	

SECTIONS	
 Sec	Mat	Section	I-2	A	A-3	
 No	No	Description	[cm^4]	[cm^2]	[cm^2]	
 1	1	Rectangle 160/320	43690.70	512.000		

ELEMENTS	
 Elem	Elem	Nodes	Beta	Section	Hinge	Part	Length	Elem	
 No	Type	Begin	End	[°]	Begin	End	Begin	End	No	[m]	Location	
 1	Beam	1	4	0.0	1	1	-	-	-	0.512	GENL	
 2	Beam	2	8	0.0	1	1	-	-	-	0.783	GENL	
 3	Beam	4	5	0.0	1	1	-	-	-	0.512	GENL	
 4	Beam	5	6	0.0	1	1	-	-	-	0.512	GENL	
 5	Beam	6	7	0.0	1	1	-	-	-	0.512	GENL	
 6	Beam	7	2	0.0	1	1	-	-	-	0.512	GENL	
 7	Beam	8	9	0.0	1	1	-	-	-	0.783	GENL	
 8	Beam	9	10	0.0	1	1	-	-	-	0.783	GENL	
 9	Beam	10	11	0.0	1	1	-	-	-	0.783	GENL	
 10	Beam	11	3	0.0	1	1	-	-	-	0.783	GENL	

SUPPORTS	
 Support	Supported	Rotation [°]	Fixed Support/Support Spring [kN/m] [kNm/rad]	
 No	Nodes	Alpha	Beta	in X	in Y	in Z	ar X	ar Y	ar Z	
 1	1	0.0	0.0	Yes	Yes	Yes	Yes	No	Yes	
 2	3	0.0	0.0	Yes	Yes	Yes	Yes	No	Yes	

GENERAL DATA	
 LS No	LS Description	Factor	Combination Type	Dead Weight	
 1	Dead Weight	1.00	Permanent	1.00	
 2	Snow	1.00	Variable	-	

ELEMENT LOADS	LS 1	
 	Loaded	Type	Load	Parameters [kN, kNm, m, °C, kN/m, kNm/m]	
 No	Elements	No	Direction	P-1				
 1	1-10	1	G	2.000				

ELEMENT LOADS	LS 2	
 	Loaded	Type	Load	Parameters [kN, kNm, m, °C, kN/m, kNm/m]	
 No	Elements	No	Direction	P-1				
 1	1-10	1	Z	3.400				

LS GROUPS	
 			Coefficient		
 LG No	LG Description	Factor	Gamma-M	Load Systems in LG	
 1		1.00	1.10	LS1 + LS2	
 2		1.00	1.10	1.30*LS1 + 1.50*LS2	

INTERNAL FORCES BY ELEMENT	
 Elem	LS/LG 	Node	x	Forces [kN]	Moments [kNm]	
 No	No	No	[m]	N	V-2	V-3	T	M-2	M-3	
     1	LS1	      1	    .00	  -12.87	     .00	     .06	     .00	     .00	     .00	
      		      4	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Max  N 	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Min  N 	    .00	  -12.87	     .00	     .06	     .00	     .00	     .00	
      		Max V-3	    .00	  -12.87	     .00	     .06	     .00	     .00	     .00	
      		Min V-3	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Max M-2	    .05	  -12.76	     .00	     .01	     .00	     .00	     .00	
      		Min M-2	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      	LS2	      1	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		      4	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Max  N 	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Min  N 	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		Max V-3	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		Min V-3	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Max M-2	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		Min M-2	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      	LG1	      1	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		      4	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Max  N 	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Min  N 	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		Max V-3	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		Min V-3	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Max M-2	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		Min M-2	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      	LG2	      1	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		      4	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Max  N 	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Min  N 	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		Max V-3	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		Min V-3	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Max M-2	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		Min M-2	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
     2	LS1	      2	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      		      8	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Max  N 	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Min  N 	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      		Max V-3	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      		Min V-3	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Max M-2	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Min M-2	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      	LS2	      2	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      		      8	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Max  N 	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Min  N 	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      		Max V-3	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      		Min V-3	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Max M-2	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Min M-2	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      	LG1	      2	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      		      8	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Max  N 	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Min  N 	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      		Max V-3	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      		Min V-3	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Max M-2	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Min M-2	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      	LG2	      2	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
      		      8	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Max  N 	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Min  N 	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
      		Max V-3	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
      		Min V-3	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Max M-2	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Min M-2	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
     3	LS1	      4	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		      5	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Max  N 	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Min  N 	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Max V-3	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Min V-3	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Max M-2	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Min M-2	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      	LS2	      4	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		      5	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Max  N 	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Min  N 	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Max V-3	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Min V-3	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Max M-2	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Min M-2	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      	LG1	      4	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		      5	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Max  N 	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Min  N 	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Max V-3	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Min V-3	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Max M-2	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Min M-2	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      	LG2	      4	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		      5	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Max  N 	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Min  N 	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Max V-3	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Min V-3	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Max M-2	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Min M-2	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
     4	LS1	      5	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		      6	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Max  N 	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Min  N 	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Max V-3	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Min V-3	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Max M-2	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Min M-2	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      	LS2	      5	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		      6	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Max  N 	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Min  N 	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Max V-3	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Min V-3	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Max M-2	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Min M-2	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      	LG1	      5	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		      6	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Max  N 	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Min  N 	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Max V-3	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Min V-3	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Max M-2	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Min M-2	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      	LG2	      5	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		      6	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Max  N 	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Min  N 	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Max V-3	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Min V-3	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Max M-2	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Min M-2	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
     5	LS1	      6	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		      7	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Max  N 	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Min  N 	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Max V-3	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Min V-3	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Max M-2	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Min M-2	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      	LS2	      6	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		      7	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Max  N 	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Min  N 	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Max V-3	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Min V-3	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Max M-2	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Min M-2	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      	LG1	      6	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		      7	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Max  N 	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Min  N 	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Max V-3	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Min V-3	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Max M-2	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Min M-2	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      	LG2	      6	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		      7	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Max  N 	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Min  N 	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Max V-3	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Min V-3	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Max M-2	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Min M-2	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
     6	LS1	      7	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		      2	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      		Max  N 	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      		Min  N 	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Max V-3	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Min V-3	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      		Max M-2	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Min M-2	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      	LS2	      7	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		      2	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      		Max  N 	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      		Min  N 	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Max V-3	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Min V-3	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      		Max M-2	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Min M-2	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      	LG1	      7	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		      2	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      		Max  N 	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      		Min  N 	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Max V-3	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Min V-3	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      		Max M-2	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Min M-2	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      	LG2	      7	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		      2	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
      		Max  N 	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
      		Min  N 	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Max V-3	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Min V-3	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
      		Max M-2	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Min M-2	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
     7	LS1	      8	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		      9	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Max  N 	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Min  N 	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Max V-3	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Min V-3	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Max M-2	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Min M-2	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      	LS2	      8	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		      9	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Max  N 	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Min  N 	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Max V-3	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Min V-3	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Max M-2	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Min M-2	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      	LG1	      8	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		      9	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Max  N 	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Min  N 	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Max V-3	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Min V-3	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Max M-2	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Min M-2	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      	LG2	      8	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		      9	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Max  N 	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Min  N 	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Max V-3	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Min V-3	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Max M-2	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Min M-2	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
     8	LS1	      9	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		     10	    .78	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Max  N 	    .78	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Min  N 	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Max V-3	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Min V-3	    .78	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Max M-2	    .70	   -5.07	     .00	     .01	     .00	    2.99	     .00	
      		Min M-2	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      	LS2	      9	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		     10	    .78	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Max  N 	    .78	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Min  N 	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Max V-3	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Min V-3	    .78	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Max M-2	    .70	   -6.15	     .00	    -.05	     .00	    4.51	     .00	
      		Min M-2	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      	LG1	      9	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		     10	    .78	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Max  N 	    .78	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Min  N 	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Max V-3	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Min V-3	    .78	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Max M-2	    .70	  -11.23	     .00	    -.04	     .00	    7.52	     .00	
      		Min M-2	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      	LG2	      9	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		     10	    .78	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Max  N 	    .78	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Min  N 	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Max V-3	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Min V-3	    .78	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Max M-2	    .70	  -15.84	     .00	    -.07	     .00	   10.70	     .00	
      		Min M-2	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
     9	LS1	     10	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		     11	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Max  N 	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Min  N 	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Max V-3	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Min V-3	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Max M-2	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Min M-2	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      	LS2	     10	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		     11	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Max  N 	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Min  N 	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Max V-3	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Min V-3	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Max M-2	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Min M-2	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      	LG1	     10	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		     11	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Max  N 	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Min  N 	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Max V-3	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Min V-3	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Max M-2	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Min M-2	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      	LG2	     10	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		     11	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Max  N 	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Min  N 	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Max V-3	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Min V-3	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Max M-2	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Min M-2	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
    10	LS1	     11	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		      3	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      		Max  N 	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      		Min  N 	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Max V-3	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Min V-3	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      		Max M-2	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Min M-2	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      	LS2	     11	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		      3	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      		Max  N 	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      		Min  N 	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Max V-3	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Min V-3	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      		Max M-2	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Min M-2	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      	LG1	     11	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		      3	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      		Max  N 	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      		Min  N 	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Max V-3	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Min V-3	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      		Max M-2	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Min M-2	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      	LG2	     11	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		      3	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
      		Max  N 	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
      		Min  N 	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Max V-3	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Min V-3	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
      		Max M-2	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Min M-2	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	

INTERNAL FORCES BY SECTION	
 Elem	LS/LG 	Node	x	Forces [kN]	Moments [kNm]	
 No	No	No	[m]	N	V-2	V-3	T	M-2	M-3	
 Section No 1: Rectangle 160/320	
     1	LS1	      1	    .00	  -12.87	     .00	     .06	     .00	     .00	     .00	
      		      4	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Max  N 	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Min  N 	    .00	  -12.87	     .00	     .06	     .00	     .00	     .00	
      		Max V-3	    .00	  -12.87	     .00	     .06	     .00	     .00	     .00	
      		Min V-3	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Max M-2	    .05	  -12.76	     .00	     .01	     .00	     .00	     .00	
      		Min M-2	    .51	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      	LS2	      1	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		      4	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Max  N 	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Min  N 	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		Max V-3	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		Min V-3	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Max M-2	    .00	  -13.51	     .00	    -.83	     .00	     .00	     .00	
      		Min M-2	    .51	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      	LG1	      1	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		      4	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Max  N 	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Min  N 	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		Max V-3	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		Min V-3	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Max M-2	    .00	  -26.38	     .00	    -.79	     .00	     .00	     .00	
      		Min M-2	    .51	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      	LG2	      1	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		      4	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Max  N 	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Min  N 	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		Max V-3	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		Min V-3	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Max M-2	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
      		Min M-2	    .51	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
     2	LS1	      2	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      		      8	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Max  N 	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Min  N 	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      		Max V-3	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      		Min V-3	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Max M-2	    .78	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Min M-2	    .00	   -6.05	     .00	    5.04	     .00	   -2.74	     .00	
      	LS2	      2	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      		      8	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Max  N 	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Min  N 	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      		Max V-3	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      		Min V-3	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Max M-2	    .78	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Min M-2	    .00	   -7.59	     .00	    7.40	     .00	   -3.84	     .00	
      	LG1	      2	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      		      8	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Max  N 	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Min  N 	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      		Max V-3	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      		Min V-3	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Max M-2	    .78	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Min M-2	    .00	  -13.65	     .00	   12.45	     .00	   -6.59	     .00	
      	LG2	      2	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
      		      8	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Max  N 	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Min  N 	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
      		Max V-3	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
      		Min V-3	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Max M-2	    .78	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Min M-2	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
     3	LS1	      4	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		      5	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Max  N 	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Min  N 	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Max V-3	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Min V-3	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Max M-2	    .00	  -11.81	     .00	    -.40	     .00	    -.09	     .00	
      		Min M-2	    .51	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      	LS2	      4	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		      5	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Max  N 	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Min  N 	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Max V-3	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Min V-3	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Max M-2	    .00	  -12.88	     .00	   -1.10	     .00	    -.50	     .00	
      		Min M-2	    .51	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      	LG1	      4	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		      5	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Max  N 	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Min  N 	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Max V-3	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Min V-3	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Max M-2	    .00	  -24.69	     .00	   -1.51	     .00	    -.59	     .00	
      		Min M-2	    .51	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      	LG2	      4	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		      5	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Max  N 	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Min  N 	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Max V-3	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Min V-3	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Max M-2	    .00	  -34.68	     .00	   -2.19	     .00	    -.87	     .00	
      		Min M-2	    .51	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
     4	LS1	      5	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		      6	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Max  N 	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Min  N 	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Max V-3	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Min V-3	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Max M-2	    .00	  -10.74	     .00	    -.85	     .00	    -.40	     .00	
      		Min M-2	    .51	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      	LS2	      5	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		      6	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Max  N 	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Min  N 	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Max V-3	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Min V-3	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Max M-2	    .00	  -12.25	     .00	   -1.37	     .00	   -1.13	     .00	
      		Min M-2	    .51	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      	LG1	      5	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		      6	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Max  N 	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Min  N 	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Max V-3	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Min V-3	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Max M-2	    .00	  -23.01	     .00	   -2.22	     .00	   -1.54	     .00	
      		Min M-2	    .51	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      	LG2	      5	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		      6	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Max  N 	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Min  N 	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Max V-3	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Min V-3	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Max M-2	    .00	  -32.36	     .00	   -3.17	     .00	   -2.24	     .00	
      		Min M-2	    .51	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
     5	LS1	      6	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		      7	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Max  N 	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Min  N 	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Max V-3	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Min V-3	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Max M-2	    .00	   -9.68	     .00	   -1.30	     .00	    -.95	     .00	
      		Min M-2	    .51	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      	LS2	      6	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		      7	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Max  N 	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Min  N 	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Max V-3	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Min V-3	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Max M-2	    .00	  -11.63	     .00	   -1.63	     .00	   -1.89	     .00	
      		Min M-2	    .51	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      	LG1	      6	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		      7	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Max  N 	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Min  N 	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Max V-3	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Min V-3	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Max M-2	    .00	  -21.32	     .00	   -2.93	     .00	   -2.86	     .00	
      		Min M-2	    .51	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      	LG2	      6	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		      7	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Max  N 	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Min  N 	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Max V-3	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Min V-3	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Max M-2	    .00	  -30.04	     .00	   -4.14	     .00	   -4.11	     .00	
      		Min M-2	    .51	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
     6	LS1	      7	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		      2	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      		Max  N 	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      		Min  N 	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Max V-3	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Min V-3	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      		Max M-2	    .00	   -8.62	     .00	   -1.75	     .00	   -1.73	     .00	
      		Min M-2	    .51	   -7.56	     .00	   -2.20	     .00	   -2.74	     .00	
      	LS2	      7	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		      2	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      		Max  N 	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      		Min  N 	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Max V-3	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Min V-3	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      		Max M-2	    .00	  -11.00	     .00	   -1.90	     .00	   -2.80	     .00	
      		Min M-2	    .51	  -10.38	     .00	   -2.16	     .00	   -3.84	     .00	
      	LG1	      7	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		      2	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      		Max  N 	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      		Min  N 	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Max V-3	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Min V-3	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      		Max M-2	    .00	  -19.63	     .00	   -3.64	     .00	   -4.55	     .00	
      		Min M-2	    .51	  -17.94	     .00	   -4.35	     .00	   -6.59	     .00	
      	LG2	      7	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		      2	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
      		Max  N 	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
      		Min  N 	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Max V-3	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Min V-3	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
      		Max M-2	    .00	  -27.72	     .00	   -5.11	     .00	   -6.48	     .00	
      		Min M-2	    .51	  -25.40	     .00	   -6.07	     .00	   -9.34	     .00	
     7	LS1	      8	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		      9	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Max  N 	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Min  N 	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Max V-3	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      		Min V-3	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Max M-2	    .78	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Min M-2	    .00	   -5.71	     .00	    3.30	     .00	     .52	     .00	
      	LS2	      8	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		      9	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Max  N 	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Min  N 	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Max V-3	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      		Min V-3	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Max M-2	    .78	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Min M-2	    .00	   -7.10	     .00	    4.83	     .00	     .95	     .00	
      	LG1	      8	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		      9	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Max  N 	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Min  N 	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Max V-3	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      		Min V-3	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Max M-2	    .78	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Min M-2	    .00	  -12.81	     .00	    8.15	     .00	    1.48	     .00	
      	LG2	      8	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		      9	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Max  N 	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Min  N 	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Max V-3	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
      		Min V-3	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Max M-2	    .78	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Min M-2	    .00	  -18.08	     .00	   11.58	     .00	    2.12	     .00	
     8	LS1	      9	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		     10	    .78	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Max  N 	    .78	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Min  N 	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Max V-3	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      		Min V-3	    .78	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Max M-2	    .70	   -5.07	     .00	     .01	     .00	    2.99	     .00	
      		Min M-2	    .00	   -5.37	     .00	    1.57	     .00	    2.43	     .00	
      	LS2	      9	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		     10	    .78	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Max  N 	    .78	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Min  N 	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Max V-3	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      		Min V-3	    .78	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Max M-2	    .70	   -6.15	     .00	    -.05	     .00	    4.51	     .00	
      		Min M-2	    .00	   -6.60	     .00	    2.26	     .00	    3.73	     .00	
      	LG1	      9	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		     10	    .78	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Max  N 	    .78	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Min  N 	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Max V-3	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      		Min V-3	    .78	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Max M-2	    .70	  -11.23	     .00	    -.04	     .00	    7.52	     .00	
      		Min M-2	    .00	  -11.98	     .00	    3.84	     .00	    6.18	     .00	
      	LG2	      9	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		     10	    .78	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Max  N 	    .78	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Min  N 	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Max V-3	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
      		Min V-3	    .78	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Max M-2	    .70	  -15.84	     .00	    -.07	     .00	   10.70	     .00	
      		Min M-2	    .00	  -16.90	     .00	    5.46	     .00	    8.80	     .00	
     9	LS1	     10	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		     11	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Max  N 	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Min  N 	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Max V-3	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Min V-3	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Max M-2	    .00	   -5.04	     .00	    -.17	     .00	    2.98	     .00	
      		Min M-2	    .78	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      	LS2	     10	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		     11	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Max  N 	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Min  N 	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Max V-3	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Min V-3	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Max M-2	    .00	   -6.10	     .00	    -.30	     .00	    4.50	     .00	
      		Min M-2	    .78	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      	LG1	     10	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		     11	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Max  N 	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Min  N 	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Max V-3	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Min V-3	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Max M-2	    .00	  -11.15	     .00	    -.47	     .00	    7.50	     .00	
      		Min M-2	    .78	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      	LG2	     10	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		     11	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Max  N 	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Min  N 	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Max V-3	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Min V-3	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Max M-2	    .00	  -15.72	     .00	    -.68	     .00	   10.67	     .00	
      		Min M-2	    .78	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
    10	LS1	     11	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		      3	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      		Max  N 	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      		Min  N 	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Max V-3	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Min V-3	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      		Max M-2	    .00	   -4.70	     .00	   -1.90	     .00	    2.17	     .00	
      		Min M-2	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
      	LS2	     11	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		      3	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      		Max  N 	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      		Min  N 	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Max V-3	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Min V-3	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      		Max M-2	    .00	   -5.60	     .00	   -2.87	     .00	    3.25	     .00	
      		Min M-2	    .78	   -5.11	     .00	   -5.44	     .00	     .00	     .00	
      	LG1	     11	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		      3	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      		Max  N 	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      		Min  N 	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Max V-3	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Min V-3	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      		Max M-2	    .00	  -10.31	     .00	   -4.79	     .00	    5.44	     .00	
      		Min M-2	    .78	   -9.48	     .00	   -9.09	     .00	     .00	     .00	
      	LG2	     11	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		      3	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
      		Max  N 	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
      		Min  N 	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Max V-3	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Min V-3	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
      		Max M-2	    .00	  -14.53	     .00	   -6.81	     .00	    7.73	     .00	
      		Min M-2	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
    10	LS1	MAX  N 	    .78	   -4.37	     .00	   -3.64	     .00	     .00	     .00	
     1	LG2	MIN  N 	    .00	  -37.00	     .00	   -1.21	     .00	     .00	     .00	
     2	LG2	MAX V-3	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	
    10	LG2	MIN V-3	    .78	  -13.35	     .00	  -12.92	     .00	     .00	     .00	
     8	LG2	MAX M-2	    .70	  -15.84	     .00	    -.07	     .00	   10.70	     .00	
     2	LG2	MIN M-2	    .00	  -19.27	     .00	   17.68	     .00	   -9.34	     .00	

SUPPORT FORCES AND SUPPORT MOMENTS	
 Node	LS/LG 	Support Forces [kN]	Support Moments [kNm]	
 No	No	P-X	P-Y	P-Z	M-X	M-Y	M-Z	
     1	LS1	    -4.979	      .000	    11.868	      .000	      .000	      .000	
      	LS2	    -6.048	      .000	    12.106	      .000	      .000	      .000	
      	LG1	   -11.033	      .000	    23.977	      .000	      .000	      .000	
      	LG2	   -15.558	      .000	    33.594	      .000	      .000	      .000	
     3	LS1	     4.979	      .000	     2.740	      .000	      .000	      .000	
      	LS2	     6.048	      .000	     4.367	      .000	      .000	      .000	
      	LG1	    11.033	      .000	     7.103	      .000	      .000	      .000	
      	LG2	    15.558	      .000	    10.106	      .000	      .000	      .000	
 	LS1	      .000	      .000	    14.608				
 		      .000	      .000	    14.608				
 	LS2	      .000	      .000	    16.473				
 		      .000	      .000	    16.473				
 	LG1	      .000	      .000	    31.081				
 		      .000	      .000	    31.081				
 	LG2	      .000	      .000	    43.699				
 		      .000	      .000	    43.699				

GLOBAL NODE DEFORMATIONS	
 Node	LS/LG 	Deformations [mm]	Rotations [mrad]	
 No	No	u-X	u-Y	u-Z	phi-X	phi-Y	phi-Z	
     1	LS1	    .00000	    .00000	    .00000	    .00000	    .08605	    .00000	
      	LS2	    .00000	    .00000	    .00000	    .00000	    .22985	    .00000	
      	LG1	    .00000	    .00000	    .00000	    .00000	    .35034	    .00000	
      	LG2	    .00000	    .00000	    .00000	    .00000	    .50805	    .00000	
     2	LS1	    .05083	    .00000	    .07199	    .00000	   -.38798	    .00000	
      	LS2	    .06145	    .00000	    .08503	    .00000	   -.64042	    .00000	
      	LG1	    .12358	    .00000	    .17279	    .00000	  -1.13555	    .00000	
      	LG2	    .17423	    .00000	    .24338	    .00000	  -1.62018	    .00000	
     3	LS1	    .00000	    .00000	    .00000	    .00000	    .80154	    .00000	
      	LS2	    .00000	    .00000	    .00000	    .00000	   1.21005	    .00000	
      	LG1	    .00000	    .00000	    .00000	    .00000	   2.21922	    .00000	
      	LG2	    .00000	    .00000	    .00000	    .00000	   3.15577	    .00000	
     4	LS1	   -.04467	    .00000	   -.00679	    .00000	    .08347	    .00000	
      	LS2	   -.10909	    .00000	   -.03330	    .00000	    .20470	    .00000	
      	LG1	   -.17041	    .00000	   -.04463	    .00000	    .31941	    .00000	
      	LG2	   -.24645	    .00000	   -.06573	    .00000	    .46200	    .00000	
     5	LS1	   -.08364	    .00000	   -.01221	    .00000	    .05937	    .00000	
      	LS2	   -.19256	    .00000	   -.05634	    .00000	    .11957	    .00000	
      	LG1	   -.30598	    .00000	   -.07630	    .00000	    .19804	    .00000	
      	LG2	   -.44168	    .00000	   -.11223	    .00000	    .28462	    .00000	
     6	LS1	   -.10098	    .00000	   -.00949	    .00000	   -.01086	    .00000	
      	LS2	   -.21874	    .00000	   -.05567	    .00000	   -.04000	    .00000	
      	LG1	   -.35402	    .00000	   -.07264	    .00000	   -.05653	    .00000	
      	LG2	   -.51002	    .00000	   -.10737	    .00000	   -.08272	    .00000	
     7	LS1	   -.06919	    .00000	    .01304	    .00000	   -.15178	    .00000	
      	LS2	   -.14917	    .00000	   -.01496	    .00000	   -.28851	    .00000	
      	LG1	   -.24177	    .00000	   -.00275	    .00000	   -.48691	    .00000	
      	LG2	   -.34825	    .00000	   -.00732	    .00000	   -.69832	    .00000	
     8	LS1	    .11932	    .00000	    .46846	    .00000	   -.55037	    .00000	
      	LS2	    .17201	    .00000	    .70934	    .00000	   -.84812	    .00000	
      	LG1	    .32125	    .00000	   1.29938	    .00000	  -1.54324	    .00000	
      	LG2	    .45603	    .00000	   1.84794	    .00000	  -2.19626	    .00000	
     9	LS1	    .17831	    .00000	    .81341	    .00000	   -.29114	    .00000	
      	LS2	    .26419	    .00000	   1.23515	    .00000	   -.43922	    .00000	
      	LG1	    .48810	    .00000	   2.26022	    .00000	   -.80590	    .00000	
      	LG2	    .69362	    .00000	   3.21484	    .00000	  -1.14606	    .00000	
    10	LS1	    .18146	    .00000	    .86777	    .00000	    .16825	    .00000	
      	LS2	    .27053	    .00000	   1.31430	    .00000	    .25857	    .00000	
      	LG1	    .49862	    .00000	   2.40750	    .00000	    .47102	    .00000	
      	LG2	    .70873	    .00000	   3.42401	    .00000	    .67028	    .00000	
    11	LS1	    .11547	    .00000	    .56278	    .00000	    .60631	    .00000	
      	LS2	    .17240	    .00000	    .85064	    .00000	    .91756	    .00000	
      	LG1	    .31756	    .00000	   1.55936	    .00000	   1.68132	    .00000	
      	LG2	    .45140	    .00000	   2.21757	    .00000	   2.39117	    .00000	
  Maxi	LS1	    .18146	    .00000	    .86777	    .00000	    .80154	    .00000	
  Mini	LS1	   -.10098	    .00000	   -.01221	    .00000	   -.55037	    .00000	
  Maxi	LS2	    .27053	    .00000	   1.31430	    .00000	   1.21005	    .00000	
  Mini	LS2	   -.21874	    .00000	   -.05634	    .00000	   -.84812	    .00000	
  Maxi	LG1	    .49862	    .00000	   2.40750	    .00000	   2.21922	    .00000	
  Mini	LG1	   -.35402	    .00000	   -.07630	    .00000	  -1.54324	    .00000	
  Maxi	LG2	    .70873	    .00000	   3.42401	    .00000	   3.15577	    .00000	
  Mini	LG2	   -.51002	    .00000	   -.11223	    .00000	  -2.19626	    .00000	

GLOBAL ELEMENT DEFORMATIONS	
 Elem	LS/LG 	Node	x	Element Deformations [mm]	
 No	No	No	[m]	u-X	u-Y	u-Z	
     1	LS1	      1	     .00	    .00000	    .00000	    .00000	
      		      4	     .51	   -.04467	    .00000	   -.00679	
      	LS2	      1	     .00	    .00000	    .00000	    .00000	
      		      4	     .51	   -.10909	    .00000	   -.03330	
      	LG1	      1	     .00	    .00000	    .00000	    .00000	
      		      4	     .51	   -.17041	    .00000	   -.04463	
      	LG2	      1	     .00	    .00000	    .00000	    .00000	
      		      4	     .51	   -.24645	    .00000	   -.06573	
     2	LS1	      2	     .00	    .05083	    .00000	    .07199	
      		      8	     .78	    .11932	    .00000	    .46846	
      	LS2	      2	     .00	    .06145	    .00000	    .08503	
      		      8	     .78	    .17201	    .00000	    .70934	
      	LG1	      2	     .00	    .12358	    .00000	    .17279	
      		      8	     .78	    .32125	    .00000	   1.29938	
      	LG2	      2	     .00	    .17423	    .00000	    .24338	
      		      8	     .78	    .45603	    .00000	   1.84794	
     3	LS1	      4	     .00	   -.04467	    .00000	   -.00679	
      		      5	     .51	   -.08364	    .00000	   -.01221	
      	LS2	      4	     .00	   -.10909	    .00000	   -.03330	
      		      5	     .51	   -.19256	    .00000	   -.05634	
      	LG1	      4	     .00	   -.17041	    .00000	   -.04463	
      		      5	     .51	   -.30598	    .00000	   -.07630	
      	LG2	      4	     .00	   -.24645	    .00000	   -.06573	
      		      5	     .51	   -.44168	    .00000	   -.11223	
     4	LS1	      5	     .00	   -.08364	    .00000	   -.01221	
      		      6	     .51	   -.10098	    .00000	   -.00949	
      	LS2	      5	     .00	   -.19256	    .00000	   -.05634	
      		      6	     .51	   -.21874	    .00000	   -.05567	
      	LG1	      5	     .00	   -.30598	    .00000	   -.07630	
      		      6	     .51	   -.35402	    .00000	   -.07264	
      	LG2	      5	     .00	   -.44168	    .00000	   -.11223	
      		      6	     .51	   -.51002	    .00000	   -.10737	
     5	LS1	      6	     .00	   -.10098	    .00000	   -.00949	
      		      7	     .51	   -.06919	    .00000	    .01304	
      	LS2	      6	     .00	   -.21874	    .00000	   -.05567	
      		      7	     .51	   -.14917	    .00000	   -.01496	
      	LG1	      6	     .00	   -.35402	    .00000	   -.07264	
      		      7	     .51	   -.24177	    .00000	   -.00275	
      	LG2	      6	     .00	   -.51002	    .00000	   -.10737	
      		      7	     .51	   -.34825	    .00000	   -.00732	
     6	LS1	      7	     .00	   -.06919	    .00000	    .01304	
      		      2	     .51	    .05083	    .00000	    .07199	
      	LS2	      7	     .00	   -.14917	    .00000	   -.01496	
      		      2	     .51	    .06145	    .00000	    .08503	
      	LG1	      7	     .00	   -.24177	    .00000	   -.00275	
      		      2	     .51	    .12358	    .00000	    .17279	
      	LG2	      7	     .00	   -.34825	    .00000	   -.00732	
      		      2	     .51	    .17423	    .00000	    .24338	
     7	LS1	      8	     .00	    .11932	    .00000	    .46846	
      		      9	     .78	    .17831	    .00000	    .81341	
      	LS2	      8	     .00	    .17201	    .00000	    .70934	
      		      9	     .78	    .26419	    .00000	   1.23515	
      	LG1	      8	     .00	    .32125	    .00000	   1.29938	
      		      9	     .78	    .48810	    .00000	   2.26022	
      	LG2	      8	     .00	    .45603	    .00000	   1.84794	
      		      9	     .78	    .69362	    .00000	   3.21484	
     8	LS1	      9	     .00	    .17831	    .00000	    .81341	
      		     10	     .78	    .18146	    .00000	    .86777	
      	LS2	      9	     .00	    .26419	    .00000	   1.23515	
      		     10	     .78	    .27053	    .00000	   1.31430	
      	LG1	      9	     .00	    .48810	    .00000	   2.26022	
      		     10	     .78	    .49862	    .00000	   2.40750	
      	LG2	      9	     .00	    .69362	    .00000	   3.21484	
      		     10	     .78	    .70873	    .00000	   3.42401	
     9	LS1	     10	     .00	    .18146	    .00000	    .86777	
      		     11	     .78	    .11547	    .00000	    .56278	
      	LS2	     10	     .00	    .27053	    .00000	   1.31430	
      		     11	     .78	    .17240	    .00000	    .85064	
      	LG1	     10	     .00	    .49862	    .00000	   2.40750	
      		     11	     .78	    .31756	    .00000	   1.55936	
      	LG2	     10	     .00	    .70873	    .00000	   3.42401	
      		     11	     .78	    .45140	    .00000	   2.21757	
    10	LS1	     11	     .00	    .11547	    .00000	    .56278	
      		      3	     .78	    .00000	    .00000	    .00000	
      	LS2	     11	     .00	    .17240	    .00000	    .85064	
      		      3	     .78	    .00000	    .00000	    .00000	
      	LG1	     11	     .00	    .31756	    .00000	   1.55936	
      		      3	     .78	    .00000	    .00000	    .00000	
      	LG2	     11	     .00	    .45140	    .00000	   2.21757	
      		      3	     .78	    .00000	    .00000	    .00000